CJ3B.info Forums

No longer active. Formerly disiscussion of the Willys Universal Jeep CJ-3B and Dispatcher DJ-3A.

Head Gasket, Oil filter canister gasket

Posted: 8:51 AM - Jul 05, 2013
wellcraft17
Two guestions, my head gasket has a metal side and a fiber side, which side up and do you apply any sealeant?

My oil filter canister is 5" in diamenter and the rubber gasket I got with my filter from NAPA is only 4.5". Where do I find the larger gasket?



Posted: 9:35 AM - Jul 05, 2013
oldtime
Metal side faced down onto the block to prevent blowout between adjacent cylinders.
Actually depends upon the specific gasket you have, but I will suggest addition of "INDIAN HEAD" gasket shellac.
Is jeep equipped with wrong oil filtration canister ?



Posted: 9:26 PM - Jul 05, 2013
wellcraft17
The cannister I think is off a military willys thus it has a larger diamenter according to some sources. I will order a filter for the military one and see if that works. It came with the willys when I purchased it.

The head gasket is a FelPro and it's for the F head


Posted: 9:08 AM - Jul 06, 2013
oldtime
You say FelPro brand ? ..... I've heard that they do not recommend use of any additional head gasket sealants



Posted: 9:16 AM - Jul 07, 2013
8305
Contacted Fel-Pro in the past by e-mail a few times, no answer, than phoned them. A guy told me to install the gasket with metal part down toward the block. He also mentioned it should be coated with copper spray.

Just removed a head after less than 3000 miles. It was already blown between #2 and #3 cylinders. The gasket was not Fel-Pro, but it was constructed similar (metal and fiber). Block and head was machined before assembly, retorqued and never been overheated. This time I will use a Fel-Pro, hopefully with more success.
I think those designers should have designed the exhaust valves in 2 and 3 cyls. further apart...



Posted: 1:15 PM - Jul 07, 2013
oldtime
wrote:I think those designers should have designed the exhaust valves in 2 and 3 cyls. further apart...


Yes I agree, IMHO that seems to be the main design flaw of the 134 engines.

